**Firmware upgrade**

Step1. Connect the R7 Ring Scanner with PC via micro-USB and open the power.

Step2. Open the upgrade program ‘Update\_V1.5.2\_EN.exe’



Step 3. Scan the following barcode to activate R7 into the update mode.



Step 4. Select the bin file-V3.8 and choose USB update.





Step 5. Waiting for completion.

